## DESCRIPTION

r.buildvrt builds a virtual raster (VRT) that is a mosaic of the list of input raster maps. The purpose of such a VRT is to provide fast access to small subsets of the VRT, also with multiple simultaneous read requests.

## NOTES

r.buildvrt creates a list of raster maps that can be located in different mapsets. The output is a read-only link to the original raster maps which is only valid if the original raster maps remain in the originally indicated mapset. A VRT can also be built from raster maps registered with r.external.

Reading the whole VRT is slower than reading the equivalent single raster map. Only reading small parts of the VRT provides a performance benefit.

A GRASS virtual raster can be regarded as a simplified version of GDAL's virtual raster format. The GRASS equivalent is simpler because issues like nodata, projection, resolution, resampling, masking are already handled by native GRASS raster routines.

## EXAMPLES

### VRT from a DEM in the North Carolina sample dataset

    # set the region
    g.region raster=elev_state_500m -p
    # higher resolution
    g.region res=50 -p
    # resample the DEM to 50 meter
    r.resamp.interp input=elev_state_500m output=elev_state_50m method=bilinear
    # create tiles
    r.tile input=elev_state_50m output=elev_state_50m_tile_ width=1000 height=1000 overlap=0
    # dump list of tiles to a file
    g.list type=raster pattern=elev_state_50m_tile_* output=tilelist
    # build a vrt
    r.buildvrt file=tilelist output=elev_state_50m_vrt

## SEE ALSO

r.tile, r.patch, r.external

The equivalent GDAL utility gdalbuildvrt

## AUTHOR

Markus Metz

Last changed: $Date$