## DESCRIPTION

t.rast.to.vect is designed to convert a space time raster dataset into a space time vector dataset. This module works as a front-end to r.to.vect and therefore supports all parameter of this module. Hence, all raster map layers in a space time raster dataset are passed to r.to.vect that converts them into vector map layers (using point,line or area as conversion criteria). Please refer to the r.to.vect documentation for a detailed description of the raster to vector conversion options. The new generated vector map layers will be registered in the output space time vector dataset, using the same time stamps as their raster map layer origins.

This module supports the parallel processing of r.to.vect module instances. The number of parallel processes can be set with the nprocs option. However, this will only work in conjunction with the -t flag, that avoids the creation of attribute tables. The parallel creation of attribute tables is not supported.

The where option allows selecting subsets of the input space time raster dataset.

The flag -n can be used to force the registration of empty vector map layers. Empty vector maps may occur in case that empty raster map layers should be converted into vector map layers.

## SEE ALSO

r.to.vect, t.rast.db.select, t.info

## AUTHOR

Sören Gebbert, Geoinformatikbüro Dassau